Port Log

Use the menu option 'Port Log' in the menu 'Tools' to bring up the following dialog:

The 'Port Log' dialog displays all UECP commands, sent or received through the serial device, in hexadecimal notation. '->' indicates that the data was sent to the Encoder, '<-' means the data was received. Use the 'Clear' Button to delete all entries in the list. The 'Save' button will save the output to a text file.

[ Content ]
DataLog

Menu 'Tools -> Data Log' will open the following dialog:

The 'Data Log' dialog displays the data ArcosII read in from the Encoder. This data will be stored in the database. Any data that couldn't read in will be displayed as '-'. In this case the database remains unchanged for this item.

[ Content ]

Suggestions and comments are welcome: support@2wcom.com