Send Data To The Encoder

To send the prepared data to the encoder, select the corresponding Checkboxes in the main window ( PS, PTY. PI... ). To finally send the data to the Encoder press the 'Send' Button. All selected data will be sent to the Encoder.

Right after pressing the 'Send' Button the following dialog will appear. The 'Send' dialog shows which data is send to the Encoder. Any occurrence of error messages will be displayed in red. The 'Port Log' window displays the data flow in hexadecimal notation.

[ Content ]
Request Data From The Encoder

Requesting data works in the same way as Sending data. Choose the Checkboxes of the data you want to request and press the 'Request' button. The output is analogous to the 'Send' dialog. The requested data will be automatically stored in the database ( existing data will be overwritten ). The 'Data Log' dialog displays the requested data in a human readable format.

[ Content ]

Suggestions and comments are welcome: support@2wcom.com